*UPDATING FIRMWARE ON THE TT4030*

*Make sure your TT4030 printer is powered off.*

*Download the firmware from the HellermannTyton tech support web page.*

*Place the file on a USB stick in a directory named* ***misc****.*

*Turn on the TT4030 printer.*

*Plug the USB stick into an open USB port on the back of the printer.*

*Using the touch screen menu on the front of the printer, tap the* ***Settings*** *icon, then the* ***Extras*** *icon.*

*Select* ***Firmware Update.***

***USB Memory*** *will already be highlighted in yellow. You should see the firmware file stored on the USB stick.*

*Tap the* ***green check mark*** *at the bottom of the screen.*

*You’ll see a progress bar as the file loads. When complete, the printer will automatically restart.*

*To see if the firmware update was successful, tap the* ***Settings*** *icon and then the* ***Info*** *icon to display the revision.*

*Version 5.1.3 or greater is needed to run print automation in Devmode.*